(module TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5E85B4CB)
  (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
  (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
  (fp_text reference REF** (at 1.27 -4.37) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal (at 1.27 4.37) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end 1.1 0) (layer F.Fab) (width 0.1))
  (fp_circle (center 2.54 0) (end 3.64 0) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 -3.25) (end 4.04 -3.25) (layer F.Fab) (width 0.1))
  (fp_line (start 4.04 -3.25) (end 4.04 3.25) (layer F.Fab) (width 0.1))
  (fp_line (start 4.04 3.25) (end -1.1 3.25) (layer F.Fab) (width 0.1))
  (fp_line (start -1.1 3.25) (end -1.5 2.85) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 2.85) (end -1.5 -3.25) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 2.85) (end 4.04 2.85) (layer F.Fab) (width 0.1))
  (fp_line (start -1.62 2.85) (end 4.16 2.85) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.5 -2.25) (end 4.04 -2.25) (layer F.Fab) (width 0.1))
  (fp_line (start -1.62 -2.25) (end 4.16 -2.25) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.62 -3.37) (end 4.16 -3.37) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.62 3.37) (end 4.16 3.37) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.62 -3.37) (end -1.62 3.37) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.16 -3.37) (end 4.16 3.37) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.835 -0.7) (end -0.701 0.835) (layer F.Fab) (width 0.1))
  (fp_line (start 0.701 -0.835) (end -0.835 0.7) (layer F.Fab) (width 0.1))
  (fp_line (start 3.375 -0.7) (end 1.84 0.835) (layer F.Fab) (width 0.1))
  (fp_line (start 3.241 -0.835) (end 1.706 0.7) (layer F.Fab) (width 0.1))
  (fp_line (start -1.86 2.97) (end -1.86 3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.86 3.61) (end -1.46 3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -2 -3.75) (end -2 3.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2 3.75) (end 4.54 3.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.54 3.75) (end 4.54 -3.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.54 -3.75) (end -2 -3.75) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 1.27 2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2.54 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ${KIPRJMOD}/3D/TE_282834-2--3DModel-STEP-56544.STEP
    (offset (xyz 1.3 0 -3.6))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
