(export (version D)
  (design
    (source D:/Users/Kuba/Documents/KiCad/test/test.sch)
    (date "2015-08-27 22:45:09")
    (tool "Eeschema (2015-08-26 BZR 6129, Git 2e41367)-product")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source test.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref P9)
      (value BeagleBone_Black_Header)
      (footprint Socket_BeagleBone_Black:Socket_BeagleBone_Black)
      (libsource (lib test-cache) (part BeagleBone_Black_Header))
      (sheetpath (names /) (tstamps /))
      (tstamp 55DF7DBA))
    (comp (ref P8)
      (value BeagleBone_Black_Header)
      (footprint Socket_BeagleBone_Black:Socket_BeagleBone_Black)
      (libsource (lib test-cache) (part BeagleBone_Black_Header))
      (sheetpath (names /) (tstamps /))
      (tstamp 55DF7DE1)))
  (libparts
    (libpart (lib test-cache) (part BeagleBone_Black_Header)
      (footprints
        (fp Socket_BeagleBone_Black))
      (fields
        (field (name Reference) P)
        (field (name Value) BeagleBone_Black_Header))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))
        (pin (num 26) (name P26) (type passive))
        (pin (num 27) (name P27) (type passive))
        (pin (num 28) (name P28) (type passive))
        (pin (num 29) (name P29) (type passive))
        (pin (num 30) (name P30) (type passive))
        (pin (num 31) (name P31) (type passive))
        (pin (num 32) (name P32) (type passive))
        (pin (num 33) (name P33) (type passive))
        (pin (num 34) (name P34) (type passive))
        (pin (num 35) (name P35) (type passive))
        (pin (num 36) (name P36) (type passive))
        (pin (num 37) (name P37) (type passive))
        (pin (num 38) (name P38) (type passive))
        (pin (num 39) (name P39) (type passive))
        (pin (num 40) (name P40) (type passive))
        (pin (num 41) (name P41) (type passive))
        (pin (num 42) (name P42) (type passive))
        (pin (num 43) (name P43) (type passive))
        (pin (num 44) (name P44) (type passive))
        (pin (num 45) (name P45) (type passive))
        (pin (num 46) (name P46) (type passive)))))
  (libraries
    (library (logical test-cache)
      (uri D:\Users\Kuba\Documents\KiCad\test\test-cache.lib)))
  (nets
    (net (code 1) (name "Net-(P9-Pad39)")
      (node (ref P9) (pin 39)))
    (net (code 2) (name "Net-(P9-Pad17)")
      (node (ref P9) (pin 17)))
    (net (code 3) (name "Net-(P9-Pad27)")
      (node (ref P9) (pin 27)))
    (net (code 4) (name "Net-(P9-Pad37)")
      (node (ref P9) (pin 37)))
    (net (code 5) (name "Net-(P9-Pad18)")
      (node (ref P9) (pin 18)))
    (net (code 6) (name "Net-(P9-Pad28)")
      (node (ref P9) (pin 28)))
    (net (code 7) (name "Net-(P9-Pad38)")
      (node (ref P9) (pin 38)))
    (net (code 8) (name "Net-(P9-Pad19)")
      (node (ref P9) (pin 19)))
    (net (code 9) (name "Net-(P9-Pad29)")
      (node (ref P9) (pin 29)))
    (net (code 10) (name "Net-(P9-Pad36)")
      (node (ref P9) (pin 36)))
    (net (code 11) (name "Net-(P8-Pad3)")
      (node (ref P8) (pin 3)))
    (net (code 12) (name "Net-(P8-Pad4)")
      (node (ref P8) (pin 4)))
    (net (code 13) (name "Net-(P8-Pad5)")
      (node (ref P8) (pin 5)))
    (net (code 14) (name "Net-(P8-Pad6)")
      (node (ref P8) (pin 6)))
    (net (code 15) (name "Net-(P8-Pad7)")
      (node (ref P8) (pin 7)))
    (net (code 16) (name "Net-(P8-Pad8)")
      (node (ref P8) (pin 8)))
    (net (code 17) (name "Net-(P9-Pad24)")
      (node (ref P9) (pin 24)))
    (net (code 18) (name "Net-(P9-Pad12)")
      (node (ref P9) (pin 12)))
    (net (code 19) (name "Net-(P9-Pad22)")
      (node (ref P9) (pin 22)))
    (net (code 20) (name VDD_ADC)
      (node (ref P9) (pin 32)))
    (net (code 21) (name "Net-(P9-Pad42)")
      (node (ref P9) (pin 42)))
    (net (code 22) (name "Net-(P9-Pad13)")
      (node (ref P9) (pin 13)))
    (net (code 23) (name "Net-(P9-Pad23)")
      (node (ref P9) (pin 23)))
    (net (code 24) (name "Net-(P9-Pad33)")
      (node (ref P9) (pin 33)))
    (net (code 25) (name "Net-(P9-Pad14)")
      (node (ref P9) (pin 14)))
    (net (code 26) (name "Net-(P8-Pad9)")
      (node (ref P8) (pin 9)))
    (net (code 27) (name "Net-(P9-Pad15)")
      (node (ref P9) (pin 15)))
    (net (code 28) (name "Net-(P9-Pad25)")
      (node (ref P9) (pin 25)))
    (net (code 29) (name "Net-(P9-Pad35)")
      (node (ref P9) (pin 35)))
    (net (code 30) (name "Net-(P9-Pad16)")
      (node (ref P9) (pin 16)))
    (net (code 31) (name "Net-(P9-Pad26)")
      (node (ref P9) (pin 26)))
    (net (code 32) (name "Net-(P8-Pad17)")
      (node (ref P8) (pin 17)))
    (net (code 33) (name "Net-(P8-Pad44)")
      (node (ref P8) (pin 44)))
    (net (code 34) (name "Net-(P8-Pad15)")
      (node (ref P8) (pin 15)))
    (net (code 35) (name "Net-(P8-Pad25)")
      (node (ref P8) (pin 25)))
    (net (code 36) (name "Net-(P8-Pad35)")
      (node (ref P8) (pin 35)))
    (net (code 37) (name "Net-(P8-Pad45)")
      (node (ref P8) (pin 45)))
    (net (code 38) (name "Net-(P8-Pad16)")
      (node (ref P8) (pin 16)))
    (net (code 39) (name "Net-(P8-Pad26)")
      (node (ref P8) (pin 26)))
    (net (code 40) (name "Net-(P8-Pad36)")
      (node (ref P8) (pin 36)))
    (net (code 41) (name "Net-(P8-Pad46)")
      (node (ref P8) (pin 46)))
    (net (code 42) (name "Net-(P8-Pad34)")
      (node (ref P8) (pin 34)))
    (net (code 43) (name "Net-(P8-Pad27)")
      (node (ref P8) (pin 27)))
    (net (code 44) (name "Net-(P8-Pad37)")
      (node (ref P8) (pin 37)))
    (net (code 45) (name "Net-(P8-Pad18)")
      (node (ref P8) (pin 18)))
    (net (code 46) (name "Net-(P8-Pad28)")
      (node (ref P8) (pin 28)))
    (net (code 47) (name "Net-(P8-Pad38)")
      (node (ref P8) (pin 38)))
    (net (code 48) (name "Net-(P8-Pad19)")
      (node (ref P8) (pin 19)))
    (net (code 49) (name "Net-(P8-Pad29)")
      (node (ref P8) (pin 29)))
    (net (code 50) (name "Net-(P8-Pad39)")
      (node (ref P8) (pin 39)))
    (net (code 51) (name "Net-(P8-Pad22)")
      (node (ref P8) (pin 22)))
    (net (code 52) (name "Net-(P8-Pad10)")
      (node (ref P8) (pin 10)))
    (net (code 53) (name "Net-(P8-Pad20)")
      (node (ref P8) (pin 20)))
    (net (code 54) (name "Net-(P8-Pad30)")
      (node (ref P8) (pin 30)))
    (net (code 55) (name "Net-(P8-Pad40)")
      (node (ref P8) (pin 40)))
    (net (code 56) (name "Net-(P8-Pad11)")
      (node (ref P8) (pin 11)))
    (net (code 57) (name "Net-(P8-Pad21)")
      (node (ref P8) (pin 21)))
    (net (code 58) (name "Net-(P8-Pad31)")
      (node (ref P8) (pin 31)))
    (net (code 59) (name "Net-(P8-Pad41)")
      (node (ref P8) (pin 41)))
    (net (code 60) (name "Net-(P8-Pad12)")
      (node (ref P8) (pin 12)))
    (net (code 61) (name "Net-(P9-Pad41)")
      (node (ref P9) (pin 41)))
    (net (code 62) (name "Net-(P8-Pad32)")
      (node (ref P8) (pin 32)))
    (net (code 63) (name "Net-(P8-Pad42)")
      (node (ref P8) (pin 42)))
    (net (code 64) (name "Net-(P8-Pad13)")
      (node (ref P8) (pin 13)))
    (net (code 65) (name "Net-(P8-Pad23)")
      (node (ref P8) (pin 23)))
    (net (code 66) (name "Net-(P8-Pad33)")
      (node (ref P8) (pin 33)))
    (net (code 67) (name "Net-(P8-Pad43)")
      (node (ref P8) (pin 43)))
    (net (code 68) (name "Net-(P8-Pad14)")
      (node (ref P8) (pin 14)))
    (net (code 69) (name "Net-(P8-Pad24)")
      (node (ref P8) (pin 24)))
    (net (code 70) (name GNDD)
      (node (ref P9) (pin 46))
      (node (ref P9) (pin 1))
      (node (ref P9) (pin 2))
      (node (ref P9) (pin 43))
      (node (ref P8) (pin 2))
      (node (ref P9) (pin 44))
      (node (ref P9) (pin 45))
      (node (ref P8) (pin 1)))
    (net (code 71) (name +3V3)
      (node (ref P9) (pin 4))
      (node (ref P9) (pin 3)))
    (net (code 72) (name +5V)
      (node (ref P9) (pin 6))
      (node (ref P9) (pin 5)))
    (net (code 73) (name PWR_BUT)
      (node (ref P9) (pin 9)))
    (net (code 74) (name SYS_5V)
      (node (ref P9) (pin 8))
      (node (ref P9) (pin 7)))
    (net (code 75) (name SYS_RESETN)
      (node (ref P9) (pin 10)))
    (net (code 76) (name "Net-(P9-Pad20)")
      (node (ref P9) (pin 20)))
    (net (code 77) (name "Net-(P9-Pad30)")
      (node (ref P9) (pin 30)))
    (net (code 78) (name "Net-(P9-Pad40)")
      (node (ref P9) (pin 40)))
    (net (code 79) (name "Net-(P9-Pad11)")
      (node (ref P9) (pin 11)))
    (net (code 80) (name "Net-(P9-Pad21)")
      (node (ref P9) (pin 21)))
    (net (code 81) (name "Net-(P9-Pad31)")
      (node (ref P9) (pin 31)))
    (net (code 82) (name GNDA_ADC)
      (node (ref P9) (pin 34)))))